{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["SCHEDULE"],"read":"whole","date_system":"1900"}

{"sheet":"SCHEDULE","index":0,"n_rows":91,"n_cols":6,"rows_kept":91,"merged":[[3,3,3,5],[11,1,11,5],[19,1,19,5],[28,1,28,5],[33,1,33,5],[34,3,34,5],[40,1,40,5],[49,1,49,5],[55,1,55,5],[65,1,65,5],[66,3,66,5],[69,1,69,5],[76,1,76,5],[81,1,81,5]]}
[]
[null,"HOME MAINTENANCE SCHEDULE"]
[]
[null,"QUARTERLY",null,"Date last completed"]
[null,"Plumbing","Description","Date","Date2","Date3"]
[null,"Faucets and shower heads","Check interior and exterior faucets for leaks. Clean aerators. Replace washers if necessary."]
[null,"Drains","Clean with baking soda. Pour water down unused drains."]
[null,"Pipes","Inspect visible pipes for leaks."]
[null,"Kitchen and bathroom cabinets","Check under and around for leaks."]
[null,"Toilets","Check for stability and leaks."]
[null,"Water heater","Check area around water heater for leaks. If you have hard water, drain 1-2 gallons water."]
[]
[null,"Interior","Description","Date","Date2","Date3"]
[null,"Wood cabinets and trim","Apply a wood protectant."]
[null,"Interior doors","Lubricate hinges."]
[null,"Garage door","Lubricate hardware. Inspect mechanism for free travel."]
[null,"Window and door tracks","Check to see if weep holes are open. Clean out dirt and dust. Lubricate rollers and latches."]
[null,"Basement or crawl space","Check for cracks or any sign of dampness or leaks. Check for any evidence of termites or wood-eating insects."]
[null,"Ceramic tile","Check and clean grout."]
[]
[null,"Electrical and Appliances","Description","Date","Date2","Date3"]
[null,"Heating and cooling systems","Clean and replace filters if necessary."]
[null,"Kitchen exhaust fan","Remove and clean the filter. Clean accumulated grease deposits from the fan housing."]
[null,"Refrigerator","Clean dust from top. Clean refrigerator drain pan. Clean and defrost freezer if necessary."]
[null,"Dishwasher","Check for leaks."]
[null,"Wiring, electrical cords, and plugs","Check for wear or damage. Replace if necessary."]
[null,"Smoke detector","Test for proper operation and replace batteries if necessary."]
[null,"GFI outlets","Test for proper operation."]
[]
[null,"Exterior","Description","Date","Date2","Date3"]
[null,"Foundation","Inspect visible areas, vents, and ducts for cracks, leaks, or blockages."]
[null,"Landscaping","Check for proper drainage. "]
[null,"Concrete and asphalt","Clean oil and grease."]
[]
[null,"FALL",null,"Date last completed"]
[null,"Plumbing","Description","Date","Date2","Date3"]
[null,"Plumbing shut-off valves","Inspect for proper operation."]
[null,"Outside faucets","Drain."]
[null,"Water heater","Flush out hot water to remove accumulated sediment."]
[null,"Faucet aerators","Check for proper flow of water. If the flow is reduced, clean the aerator screens. During the first two months, the faucet aerators could require more frequent cleaning."]
[]
[null,"Interior","Description","Date","Date2","Date3"]
[null,"Attic","Examine for evidence of any leaks. Check insulation and remove or add if necessary. Check for evidence of birds, squirrels, raccoons, etc. Check for proper ventilation."]
[null,"Countertops","Inspect for separations at sinks and backsplash. Recaulk where required."]
[null,"Tiled areas","Inspect for loose or missing grout or caulking. Regrout or recaulk if necessary."]
[null,"Shower doors/tub enclosures","Inspect for proper fit. Adjust if necessary. Inspect caulking and recaulk if necessary."]
[null,"Weather stripping","Check caulking around windows and doors. Check window and door screens. Adjust or replace if necessary."]
[null,"Sectional garage doors","Adjust the travel and tension."]
[null,"Fireplace","Inspect flues. Clean if necessary. Inspect fireplace brick and mortar for cracks or damage. "]
[]
[null,"Electrical and appliances","Description","Date","Date2","Date3"]
[null,"Heating system","Service heating system and heat pump."]
[null,"Cooling system","Remove debris from around units and clean with garden hose. Remove window air conditioner or protect with weatherproof cover. Clean and replace filters if necessary."]
[null,"Refrigerator coils","Clean."]
[null,"Combustible appliances","Inspect and service if necessary."]
[]
[null,"Exterior","Description","Date","Date2","Date3"]
[null,"Roof","Check for leaks. Check for damaged, loose, or missing shingles. Check vents and louvers for birds, nests, squirrels, and insects. Check flashing around roof stacks, vents, and skylights for leaks."]
[null,"Chimney","Clean and check for deteriorating bricks and mortar. Check for leaks. Check for birds, nests, squirrels, and insects."]
[null,"Gutters and downspouts","Clean and check for leaks, misalignment, or damage."]
[null,"Exterior walls","Check for deteriorating bricks and mortar. Check siding for damage or rot. Check painted surfaces for flaking."]
[null,"Landscaping","Trim shrubbery around walls. Remove tree limbs, branches, or debris that can attract insects (no wood or shrubbery should be closer than 3 inches to your house). Maintain grading."]
[null,"Concrete and asphalt","Check for cracks or deterioration. Reseal or repair if necessary."]
[null,"Septic system","Examine septic system drain field for flooding and odor. Have tank pumped yearly."]
[null,"Lawn and patio furniture","Clean and store or cover with weatherproof material."]
[]
[null,"SPRING",null,"Date last completed"]
[null,"Plumbing","Description","Date","Date2","Date3"]
[null,"Water heater","Flush out hot water to remove accumulated sediment."]
[]
[null,"Interior","Description","Date","Date2","Date3"]
[null,"Attic","Examine for evidence of any leaks. Check insulation and remove or add if necessary. Check for evidence of birds, squirrels, raccoons, etc. Check for proper ventilation."]
[null,"Countertops","Inspect for separations at sinks and backsplash. Recaulk where required."]
[null,"Tiled areas","Inspect for loose or missing grout or caulking. Regrout or recaulk if necessary."]
[null,"Shower doors/tub enclosures","Inspect for proper fit. Adjust if necessary. Inspect caulking and recaulk if necessary."]
[null,"Weather stripping","Check caulking around windows and doors. Check window and door screens. Adjust or replace if necessary."]
[]
[null,"Electrical and appliances","Description","Date","Date2","Date3"]
[null,"Heating and cooling system","General furnace inspection: Look for rust, scaling on heat exchanger, and proper flame color; note odd sounds or smells; and check condition of venting. Remove debris around units."]
[null,"Circuit breakers ","Exercise."]
[null,"Refrigerator","Clean coils."]
[]
[null,"Exterior","Description","Date","Date2","Date3"]
[null,"Decks","Scrub mildewed areas and treat for water stains, mildew, and fungus."]
[null,"Roof","Clean. Check for leaks. Check for damaged, loose or missing shingles. Check vents and louvers for birds, nests, squirrels, and insects. Check flashing around roof stacks, vents, and skylights for leaks."]
[null,"Chimney","Clean and check for deteriorating bricks and mortar. Check for leaks. Check for birds, nests, squirrels, and insects."]
[null,"Gutters and downspouts","Clean and check for leaks, misalignment, or damage."]
[null,"Windows","Clean."]
[null,"Exterior walls","Check for deteriorating bricks and mortar. Check siding for damage or rot. Check painted surfaces for flaking."]
[null,"Landscaping","Trim shrubbery around walls. Remove tree limbs, branches, or debris that can attract insects (no wood or shrubbery should be closer than 3 inches to your house). Maintain grading."]
[null,"Concrete and asphalt","Check for cracks or deterioration. Reseal or repair if necessary."]